Purchased 2020

Garage2 camera stopped working late 2021? - replaced with camera purchased March 2022

url of product:
https://www.aliexpress.com/item/4000032458493.html?spm=a2g0s.9042311.0.0.b9a04c4dn3nsMk

Specifications:
·  Brand Name: REVOTECH
·  Style: Mini Camera
·  Type: IP Camera
·  Connectivity: IP/Network Wired
·  Supported Operating Systems: Windows 10
·  Supported Operating Systems: Windows Vista
·  Supported Operating Systems: Windows 8
·  Supported Operating Systems: Windows 7
·  Supported Operating Systems: Windows 98
·  Supported Operating Systems: Windows XP
·  High Definition: 3.0 Megapixels
·  Lens (mm): 3.7mm
·  Installation: Ceiling
·  Power Supply(V): DC12V/2A
·  Dimensions (L x W x D)(mm): 10.2 x 6 x 2.7cm
·  Model Number: IPIR-M
·  Network Interface: RJ-45 10/100Mb Ethernet Slot
·  Wall Bracket: Ceiling
·  Supported Mobile Systems: ios
·  Supported Mobile Systems: Android
·  IR Distance(m): 5-10m
·  Megapixels: 3MP
·  Power Consumption(W): NA
·  Storage: None
·  Alarm Action: Email Photo
·  Video Compression Format: H.264
·  Video Compression Format: H.265
·  is_customized: Yes
·  Technology: Pinhole
·  Power Supply: Normal
·  TF Card: None
·  Color: White
·  Audio Output: None
·  Minimum Illumination(Lux): NA
·  Sensor: CMOS
·  Type: CCTV Camera
·  Model: IP Camera
·  LENS: 3.7mm
·  TV Format: PAL/NTSC
·  LED: 18 IR
·  Night Vision: Yes
·  Resolution: 3MP / 1080P
·  IR Cut: Support
·  Place of Origin: Guangdong, China (Mainland)


To set ip/subnet for BlueIris at cabin
When first tried could change ip address and subnet of camera but could neither BlueIris nor the software for the camera (CMS3.0) would connect.
Then when set CMS3.0 software and then changed the IP camera it worked!
Set software:
1. Plug in camera (power & ehternet)
2. Open CMS3.0
3. Click icon (two computer monitors
4. CMS3.0 Login pop up (admin; password blank); OK
5. Set Network:
6. NIC: Local Area Connection
7. Enable DHCP: unchecked
8. IP: 10.10.10.70
9. Netmask: 255.255.255.0
10. Gateway: 0.0.0.0
11. DNS: 255.255.255.255
12. Ok

Set camera:
13. In CMS3.0 window, top left right click on the camera
14. Modify Device
15. Network
16. 


